DTI supports these following basic options. Customer can see more details in part 2.2

Column mux option

Output drive strength

Write enable

register output (with and without scanning mode)

Asynchronous write through

Clock edge

Test input

XOR

Column redundancy

Row redundancy

Output enable

Decap

Deep Nwell

VT options

Memory cell options

Synchronous write